      HUBBARD COMMUNICATIONS OFFICE

Saint Hill Manor, East Grinstead, Sussex



    HCO BULLETIN OF 10 DECEMBER 1965



Remimeo

Academy Students



             Tech Division



        E-METER DRILL COACHING



The following was submitted by Malcolm Cheminais, Supervisor on the

Saint Hill Special Briefing Course.



Here are some observations I have made on the coaching of E-Meter

drills, which I feel could be of use:



1. The coach's needle is dirty. The student's out-comm cycle has cut

his comm in some way, but PRIOR to that the coach failed to flunk

the part of the comm cycle that went out. Correct flunking by

coaches equals students with no dirty needles.



2. If a coach's TA starts climbing on a drill and the needle gets

sticky, it means that the student's comm cycle has dispersed him and

pushed him out of PT. The coach is either (1) not flunking at all,

(2) flunking the incorrect thing.



3. The correct flunking by the coach of an out-comm cycle, which has

dispersed him and pushed his TA up will always result in a TA

blowdown. If there is no blowdown, the coach has flunked the wrong

thing.



4. Needle not responding well and sensitively on assessment drills,

although the needle clean. Coach has failed to flunk TR 1 (or TR 0) 

for lack of impingement and reach.



5. Coach reaching forward and leaning on the table, means TR 1 is 

out with the student.



6. Student asking coach for considerations to get TA down, but TA 

climbing on the considerations -- the coach is cleaning a clean,

instead of flunking the out-comm cycle, which occurred earlier and

pushed his TA up.



7. Student getting coach's considerations off to clean the needle,

but needle remaining dirty -- student is cutting the coach's comm

while getting the considerations off and the coach is not picking

this up.



8. Students shouting or talking very loudly on assessment drills to

try and get the meter to read by overwhelm. The reason for this is

invariably -- "but I'm assessing the bank!" They haven't realized

that banks don't read, only thetans impinged upon by the bank -

therefore, the TR 1 must be addressed to the thetan. The meter

responds proportionately to the amount of ARC in the session.





L. RON HUBBARD

Founder



LRH:emp.gm



