      HUBBARD COMMUNICATIONS OFFICE

Saint Hill Manor, East Grinstead, Sussex



   HCO BULLETIN OF 10 DECEMBER 1976RB

         RE-REVISED 25 MAY 1980



Remimeo

All Auditors

All Intern Supervisors

All C/Ses



           URGENT - IMPORTANT



            C/S Series 99RB



     SCIENTOLOGY F/N AND TA POSITION





Through verbal tech just located, it has been found that some 

auditors have been ordered to disregard all F/Ns that were above 

3.0 or below 2.0 on the meter.



Auditors have also called F/Ns which were ARC break needles, thus 

falsely indicating to the pc.



These two actions -- disregarding actual F/Ns because the TA was

not between 2.0 and 3.0 and calling "F/Ns" that were actually ARC

break needles -- have upset many preclears.



The outnesses here are (A) not considering pc indicators as senior 

and (B) not noting pc indicators when calling an F/N and (C) 

ignoring and giving junior importance to the technology covered in 

false TAs. (See list of references at end of this HCOB or the 

Subject Index of the HCOB Volumes.)



Auditors have even been led to falsify worksheets (giving TA as in 

range when it actually was not when calling an F/N) because they 

might "get in trouble" for calling an F/N in the wrong range, such 

as 1.8 or 3.2.



The CORRECT procedure for out-of-range F/Ns is:



1. Look at the pc's indicators.



2. Call the F/N regardless of its range.



3. Mark down the ACTUAL TA position.



4. Handle the false TA at the earliest opportunity when it will not 

intrude into the current cycle on which the pc is being audited. 

(You don't interrupt a Quad R3RA, for instance, to handle false TA; 

you complete it and then, when directed by the C/S, you handle the 

false TA.)



5. On any pc you suspect has had his F/Ns disregarded because of 

false TA, you C/S for and get run a repair and rehab of this error.



E-Meter cans can monitor or change TA position when the palms are 

too dry or too wet or when the cans are too big or too small or 

when the wrong hand cream is used. The E-Meter does not read on 

hand moisture alone as was long believed by people in electronics. 

But TA depends upon resistance to electrical current in the palms, 

leads and meter, as well as its main resistance which happens to be 

mental masses or lack of them.



To simply tell some intern "Always disregard an F/N not in correct 

range" is to set him up for loses and set the pc up for crashes. 

The correct information is that an F/N which isn't in range is 

accompanied by pc indicators that indicate whether it is an F/N or 

not. AND indicates you better get the false TA handled fast as soon 

as it won't interrupt the current cycle. AND you always note where 

it F/Ned so the C/S can C/S for false TA handling.



Where an ARC break needle (which looks like an F/N) is observed, 

whether it Is in range or out of range (2.0 to 3.0 or below 2.0 or 

above 3.0) you LOOK at the pc and establish the pc's indicators 

before falsely calling an F/N. A pc who is about to cry is NOT an 

F/Ning pc, and if you indicate an F/N to that pc, you will further 

the ARC break and suppress the emotional charge that is about to 

come off.



                 REPAIR



Where the above matters have not been fully understood and errors 

have occurred on pcs, It must be assumed that:



1. Auditors have falsified their worksheets as to TA position and 

thus built up withholds and made themselves blowy.



2. That every pc who has ever had high or low TA trouble has had 

F/Ns disregarded and ARC break F/Ns falsely indicated.



3. That a briefing and drilling of all interns and auditors must 

occur on this HCOB.



4. That a brief program of cleanup of disregarded F/Ns and falsely 

called ARC break F/Ns be done on every pc.



5. That every such pc be considered as having false TA troubles and 

these must be C/Sed for and corrected.



6. That all auditors and interns be drilled on all HCOBs relating 

to pc indicators,



          SAMPLE CLEANUP C/S



Disregard TA position, use only F/Ns and pc indicators in doing 

this C/S.



1. It has been found that some of your F/Ns (release points) may 

have been disregarded by past or present auditors.



2. Have you ever felt an F/N (release point or end of an action) 

had been bypassed on your case?



3. Find and rehab the overrun of the release point to F/N. Check 

for any other bypassed F/Ns and rehab them.



4. Have you ever felt an F/N should not have been indicated by the 

auditor when it was?



5. Find the point and get in Suppress on it and complete the 

action. Check "Are there any other F/Ns which should not have been 

indicated by the auditor when they were?" and handle as above.



6. Find and run the ARC breaks bypassed, with ARC break handling.



7. Find and handle the false TA in totality.



              DIANETIC F/Ns



An F/N seen by the auditor in running R3RA is not called until the 

full Dianetic EP is reached.



An auditor running R3RA is NOT looking for F/Ns. He is looking for 

the postulate which is sitting at the bottom of the chain he is 

running.



The EP of a Dianetic chain is always always always the postulate 

coming off. The postulate is what holds the chain in its place. 

Release the postulate and the chain blows. That's it.



The auditor must recognize the postulate when the pc gives it, note 

the VGIs, call the F/N and end off auditing that chain.



An F/N seen as the incident is erasing is not called.



The pc does not have to state that the incident has erased. Once he 

has given up the postulate, the erasure has occurred. The auditor 

will see an F/N and VGIs. NOW the F/N is called. F/Ns are not 

indicated until the EP of postulate off, F/N and VGIs is reached.



It's the postulate -- not the F/N -- that we are going for in New

Era Dianetics.



               POWER F/Ns



F/Ns are disregarded in Power.



Each Power Process has its own end phenomena and is ended only when 

that is obtained.



       REFERENCE HCOBs FOR FALSE TA



Refs:

HCOB  8 June 70       LOW TA HANDLING

HCOB 16 Aug. 70R      C/S Series 15R

                      GETTING THE F/N TO THE

                      EXAMINER

HCOB 24 Oct. 71RA     FALSE TA

HCOB 12 Nov. 71RB     FALSE TA ADDITION

HCOB 15 Feb. 72R      FALSE TA ADDITION 2

HCOB 18 Feb. 72RA I   FALSE TA ADDITION 3

HCOB 16 Feb. 72       C/S Series 74

                      TALKING THE TA DOWN MODIFIED

HCOB 23 Nov. 73RB     DRY AND WET HANDS MAKE FALSE TA

HCOB 24 Nov. 73RD     C/S Series 53RL SF

                      SHORT HI-LO TA ASSESSMENT C/S

HCOB 24 Nov. 73RE     C/S SERIES 53RL LONG FORM

HCOB 19 Apr. 75       OUT-BASICS AND HOW TO GET THEM IN

HCOB 23 Apr. 75RA     VANISHING CREAM AND FALSE TA

HCOB 24 Oct. 76RA     C/S Series 96RA

                      DELIVERY REPAIR LISTS

HCOB 10 Dec. 76RB     C/S Series 99RB

                      SCIENTOLOGY F/N AND TA POSITION

HCOB 21 Jan. 77RB     FALSE TA CHECKLIST

HCOB 24 Jan. 77       TECH CORRECTION ROUNDUP

HCOB 26 Jan. 77R      FOOTPLATES USE FORBIDDEN

HCOB 30 Jan. 77R      FALSE TA DATA

HCOB  4 Dec. 77       CHECKLIST FOR SETTING UP

                      SESSIONS AND AN E-METER

HCOB 13 Jan. 77RB     HANDLING A FALSE TA

Owner's Manual for your E-Meter





        PC INDICATORS HCOBs



Refs:

HCOB 29 July 64       GOOD INDICATORS AT LOWER LEVELS

HCOB 28 Dec. 63       INDICATORS, PART ONE: GOOD INDICATORS

HCOB 23 May 71R VIII  RECOGNITION OF RIGHTNESS OF THE BEING

   Rev. 4.12.74

HCOB 22 Sept. 71      THE THREE GOLDEN RULES OF

                      THE C/S, HANDLING AUDITORS

HCOB 21 Oct. 68R      FLOATING NEEDLE





L. RON HUBBARD

Founder



Revision assisted by

LRH Technical Research

and Compilations



LRH:RTRC:djm.dd.gm



